(footprint "XFMR_DAGNALL_D3510"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DAGNALL 1VA PCB Mounted Encapsulated TransformerBody 27.5mm x 32.5mm")
	(property "Reference" "REF**"
		(at 0 -17.05001 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_DAGNALL_D3510"
		(at 0 17.05001 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "SEC"
		(at 6.07201 -6.01378 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "PRIM"
		(at -4.11665 1.72125 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "SEC"
		(at 6.07201 8.98623 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "PRIM"
		(at -4.11665 1.72125 90)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "SEC"
		(at 6.07201 8.98623 90)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "SEC"
		(at 6.07201 -6.01378 90)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -10.00001 -10.00001 90)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -10.00001 10.00001 90)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 10.00001 -10.00001 90)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at 10.00001 -5 90)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at 10.00001 5 90)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at 10.00001 10.00001 90)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
