(footprint "XFMR_MURATA_5600"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "MURATA Current Sensing Transformer, Body 16.79x8.89mm, 5600 Serie")
	(property "Reference" "REF**"
		(at 0 -5.245 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_MURATA_5600"
		(at 0 5.245 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "2"
		(at -0.49 6.322 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at 5.86 6.322 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -6.84 6.322 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -6.84 6.322 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "3"
		(at 5.86 6.322 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "2"
		(at -0.49 6.322 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -6.35 0.386)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 0 0.386)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 6.35 0.386)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
