(footprint "XFMR_MYRRA_44000_EI30x12.5"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "EI 30x12.5, 1.5VA Encapsulated Transformer 44000 Series")
	(property "Reference" "REF**"
		(at -0.3875 -17.225 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_MYRRA_44000_EI30x12.5"
		(at -0.3875 17.225 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "9"
		(at 6.44999 -4.35299 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at 6.44999 10.64701 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "7"
		(at 6.44981 5.64721 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "5"
		(at -8 10.647 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -7.97499 -9.35299 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "10"
		(at 6.44999 -9.35299 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -7.97517 -9.3528 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "7"
		(at 6.44999 5.64701 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "9"
		(at 6.44981 -4.3528 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at 6.44981 10.64721 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "10"
		(at 6.44981 -9.3528 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5"
		(at -8 10.647 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -10 -10)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -10 10)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at 10 10)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at 10 5)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "9" thru_hole circle
		(at 10 -5)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "10" thru_hole circle
		(at 10 -10)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
