(footprint "XFMR_MYRRA_44000_EI42x14.8"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "EI 42x14.8, 5VA Encapsulated Transformer Serie 44000")
	(property "Reference" "REF**"
		(at -0.00005 -23.05001 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_MYRRA_44000_EI42x14.8"
		(at -0.00005 23.0502 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "5"
		(at -10.47496 13.14702 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "10"
		(at 8.95004 -11.853 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "10"
		(at 8.94986 -11.8528 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "9"
		(at 8.94986 -6.8528 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "7"
		(at 8.94986 8.14721 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at 8.95004 13.14702 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at 8.94986 13.14721 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "9"
		(at 8.95004 -6.85299 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "5"
		(at -10.47513 13.14721 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "7"
		(at 8.95004 8.14702 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -10.47496 -11.853 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -10.47513 -11.8528 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "1" thru_hole circle
		(at -12.49997 -12.50001)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -12.49997 12.50001)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at 12.50005 12.50001)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at 12.50005 7.50001)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "9" thru_hole circle
		(at 12.50005 -7.5)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "10" thru_hole circle
		(at 12.50005 -12.50001)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
