(footprint "XFMR_MYRRA_44000_EI48-16.8"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "EI 48-16.8, 5VA Encapsulated Transformer Serie 44000")
	(property "Reference" "REF**"
		(at 0 -26.225 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_MYRRA_44000_EI48-16.8"
		(at 0 26.225 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "13"
		(at 8.94986 -6.8528 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "9"
		(at 8.95004 8.14702 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -10.47513 -11.8528 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "8"
		(at 8.94986 13.14721 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "7"
		(at -10.47513 13.14721 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "14"
		(at 8.94986 -11.8528 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "7"
		(at -10.47496 13.14702 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "8"
		(at 8.95004 13.14702 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -10.47496 -11.853 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "" np_thru_hole circle
		(at 0 -20)
		(size 2 2)
		(drill 4)
		(layers "F&B.Cu" "*.Mask")
		(solder_mask_margin 1)
		(thermal_bridge_angle 90)
	)
	(pad "" np_thru_hole circle
		(at 0 20)
		(size 2 2)
		(drill 4)
		(layers "F&B.Cu" "*.Mask")
		(solder_mask_margin 1)
		(thermal_bridge_angle 90)
	)
	(pad "1" thru_hole circle
		(at -13.75 -12.5)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at -13.75 12.5)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at 13.75 12.5)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "9" thru_hole circle
		(at 13.75 7.5)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "13" thru_hole circle
		(at 13.75 -7.5)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "14" thru_hole circle
		(at 13.75 -12.5)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
