(footprint "XFMR_MYRRA_45026"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "250V to 2x9V, UI 30, 6VA Encapsulated Transformer Serie  45000")
	(property "Reference" "REF**"
		(at 0 -22.80001 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_MYRRA_45026"
		(at 0 22.80001 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "SEC1"
		(at 18.43375 -10 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "PR2"
		(at -16.56625 9.5 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "16"
		(at 19.5 -16.853 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -20 -16.853 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "SEC2"
		(at 18.43375 10 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "5"
		(at -20 3.14701 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "12"
		(at 19.5 3.14701 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "14"
		(at 19.5 -6.85299 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "10"
		(at 19.5 13.14702 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at -20 -6.85299 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "PR1"
		(at -16.56625 -11 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "7"
		(at -20 13.14702 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "1" thru_hole circle
		(at -17.50001 -17.50001)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at -17.50001 -7.50001)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -17.50001 2.5)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at -17.50001 12.50001)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "10" thru_hole circle
		(at 17.50001 12.50001)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "12" thru_hole circle
		(at 17.50001 2.5)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "14" thru_hole circle
		(at 17.50001 -7.5)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "16" thru_hole circle
		(at 17.50001 -17.50001)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "MTG" thru_hole circle
		(at -23.75001 -18.75001)
		(size 4.8 4.8)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "MTG" thru_hole circle
		(at -23.75001 18.75001)
		(size 4.8 4.8)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "MTG" thru_hole circle
		(at 23.75001 -18.75001)
		(size 4.8 4.8)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "MTG" thru_hole circle
		(at 23.75001 18.75001)
		(size 4.8 4.8)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
