(footprint "XFMR_MYRRA_45000_UI48x26"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "UI 39x21, 30VA Encapsulated Transformer Serie 45000")
	(property "Reference" "REF**"
		(at 0 -35.75008 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_MYRRA_45000_UI48x26"
		(at 0 35.74992 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "PR1"
		(at -29.69674 -21.2 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "17"
		(at 29.56837 8.54247 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at -28.37151 -13.45753 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "9"
		(at -28.429 13.54247 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "20"
		(at 29.568375 -8.45753 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "SEC2"
		(at 30.18375 18.5 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "PR2"
		(at -29.69673 20.79999 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "14"
		(at 29.568375 23.54247 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -28.657165 -28.45753 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "SEC1"
		(at 30.18375 -13.5 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "9"
		(at -28.42864 28.54247 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "23"
		(at 29.568375 -23.45753 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "1" thru_hole circle
		(at -26.5 -28.50008)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -26.5 -23.50008)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at -26.5 -18.50008)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -26.5 -13.50008)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -26.5 -8.50008)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at -26.5 -3.50008)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at -26.5 3.49992)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at -26.5 8.49992)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "9" thru_hole circle
		(at -26.5 13.49992)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "10" thru_hole circle
		(at -26.5 18.49992)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "11" thru_hole circle
		(at -26.5 23.49992)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "12" thru_hole circle
		(at -26.5 28.49992)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "13" thru_hole circle
		(at 26.5 28.49992)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "14" thru_hole circle
		(at 26.5 23.49992)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "15" thru_hole circle
		(at 26.5 18.49992)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "16" thru_hole circle
		(at 26.5 13.49992)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "17" thru_hole circle
		(at 26.5 8.49992)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "18" thru_hole circle
		(at 26.5 3.49992)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "19" thru_hole circle
		(at 26.5 -3.50008)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "20" thru_hole circle
		(at 26.5 -8.50008)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "21" thru_hole circle
		(at 26.5 -13.5)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "22" thru_hole circle
		(at 26.5 -18.50008)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "23" thru_hole circle
		(at 26.5 -23.50008)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "24" thru_hole circle
		(at 26.5 -28.5)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "MTG" thru_hole circle
		(at -37.5 -30.00008)
		(size 5.5 5.5)
		(drill 3.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "MTG" thru_hole circle
		(at -37.5 29.99992)
		(size 5.5 5.5)
		(drill 3.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "MTG" thru_hole circle
		(at 37.5 -30.25008)
		(size 5.5 5.5)
		(drill 3.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "MTG" thru_hole circle
		(at 37.5 29.99992)
		(size 5.5 5.5)
		(drill 3.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
