(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "XFMR_PULSE_H1260NL"
  		(pin_names
  			(offset 1.27)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "TR"
  			(at 15.24 1.27 0)
  		)
  		(property "Value" "${DEVICE}"
  			(at 15.24 -24.13 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "10/100BASE-T Single Port LAN Transformer Module"
  			(at 0 0 0)
  		)
  		(symbol "XFMR_PULSE_H1260NL_1_0"
  			(text "1:1"
  				(at 10.922 -1.524 0)
  			)
  			(text "1:1"
  				(at 10.922 -14.224 0)
  			)
  			(pin bidirectional line
  				(at -5.08 -2.54 0)
  				(length 5.08)
  				(name "TD+")
  				(number "1")
  			)
  			(pin bidirectional line
  				(at -5.08 -5.08 0)
  				(length 5.08)
  				(name "TCTD")
  				(number "2")
  			)
  			(pin bidirectional line
  				(at -5.08 -7.62 0)
  				(length 5.08)
  				(name "TD-")
  				(number "3")
  			)
  			(pin bidirectional line
  				(at -5.08 -10.16 0)
  				(length 5.08)
  				(name "NC")
  				(number "4")
  			)
  			(pin bidirectional line
  				(at -5.08 -12.7 0)
  				(length 5.08)
  				(name "NC")
  				(number "5")
  			)
  			(pin bidirectional line
  				(at -5.08 -15.24 0)
  				(length 5.08)
  				(name "RD+")
  				(number "6")
  			)
  			(pin bidirectional line
  				(at -5.08 -17.78 0)
  				(length 5.08)
  				(name "RCRD")
  				(number "7")
  			)
  			(pin bidirectional line
  				(at -5.08 -20.32 0)
  				(length 5.08)
  				(name "RD-")
  				(number "8")
  			)
  			(pin bidirectional line
  				(at 35.56 -2.54 180)
  				(length 5.08)
  				(name "TX+")
  				(number "16")
  			)
  			(pin bidirectional line
  				(at 35.56 -5.08 180)
  				(length 5.08)
  				(name "CTX")
  				(number "15")
  			)
  			(pin bidirectional line
  				(at 35.56 -7.62 180)
  				(length 5.08)
  				(name "TX-")
  				(number "14")
  			)
  			(pin bidirectional line
  				(at 35.56 -10.16 180)
  				(length 5.08)
  				(name "NC")
  				(number "13")
  			)
  			(pin bidirectional line
  				(at 35.56 -12.7 180)
  				(length 5.08)
  				(name "NC")
  				(number "12")
  			)
  			(pin bidirectional line
  				(at 35.56 -15.24 180)
  				(length 5.08)
  				(name "RX+")
  				(number "11")
  			)
  			(pin bidirectional line
  				(at 35.56 -17.78 180)
  				(length 5.08)
  				(name "CRX")
  				(number "10")
  			)
  			(pin bidirectional line
  				(at 35.56 -20.32 180)
  				(length 5.08)
  				(name "RX-")
  				(number "9")
  			)
  		)
  		(embedded_fonts no)
  	)
)
