(footprint "XFMR_PULSE_H5007NL"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "10/100BASE-T Magnetics Modules, Body 12.2 x 17.53mm")
	(property "Reference" "REF**"
		(at 0 -9.74 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_PULSE_H5007NL"
		(at 0 9.74 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -7.3025 -6.985)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -7.3025 -5.715)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -7.3025 -4.445)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -7.3025 -3.175)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -7.3025 -1.905)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -7.3025 -0.635)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -7.3025 0.635)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -7.3025 1.905)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -7.3025 3.175)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -7.3025 4.445)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -7.3025 5.715)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -7.3025 6.985)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 7.3025 6.985)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 7.3025 5.715)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 7.3025 4.445)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 7.3025 3.175)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 7.3025 1.905)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 7.3025 0.635)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 7.3025 -0.635)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 7.3025 -1.905)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 7.3025 -3.175)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 7.3025 -4.445)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 7.3025 -5.715)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 7.3025 -6.985)
		(size 1.905 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
