(footprint "XFMR_PULSE_HM2108NL"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Pulse Transformer for Battery Management CMC")
	(property "Reference" "REF**"
		(at 0 -5.22492 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_PULSE_HM2108NL"
		(at 0 5.22508 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -7.825 -2.53992)
		(size 1.95 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -7.825 0.00008)
		(size 1.95 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -7.825 2.54008)
		(size 1.95 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 7.825 2.54008)
		(size 1.95 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 7.825 0.00008)
		(size 1.95 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 7.825 -2.53992)
		(size 1.95 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
