(footprint "XFMR_PULSE_HX5020FNL"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "1000 Base-T Ethernet Transformer/Choke, Body 10.92 x 27.94mm")
	(property "Reference" "REF**"
		(at -0.2425 -14.818 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_PULSE_HX5020FNL"
		(at -0.2425 14.818 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -4.7625 -12.192)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4.7625 -11.176)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.7625 -10.16)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -4.7625 -9.144)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -4.7625 -8.128)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -4.7625 -7.112)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -4.7625 -6.096)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -4.7625 -5.08)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -4.7625 -4.064)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -4.7625 -3.048)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -4.7625 -2.032)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -4.7625 -1.016)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -4.7625 0)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -4.7625 1.016)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -4.7625 2.032)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -4.7625 3.048)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -4.7625 4.064)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -4.7625 5.08)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -4.7625 6.096)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -4.7625 7.112)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -4.7625 8.128)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -4.7625 9.144)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -4.7625 10.16)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at -4.7625 11.176)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -4.7625 12.192)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 4.7625 12.192)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 4.7625 11.176)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 4.7625 10.16)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 4.7625 9.144)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 4.7625 8.128)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 4.7625 7.112)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 4.7625 6.096)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 4.7625 5.08)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 4.7625 4.064)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 4.7625 3.048)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 4.7625 2.032)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 4.7625 1.016)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 4.7625 0)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 4.7625 -1.016)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 4.7625 -2.032)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 4.7625 -3.048)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 4.7625 -4.064)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at 4.7625 -5.08)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at 4.7625 -6.096)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at 4.7625 -7.112)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at 4.7625 -8.128)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at 4.7625 -9.144)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at 4.7625 -10.16)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at 4.7625 -11.176)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at 4.7625 -12.192)
		(size 1.905 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
