(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "XFMR_PULSE_HX5020FNL"
  		(pin_names
  			(offset 1.27)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "TR"
  			(at 15.24 1.27 0)
  		)
  		(property "Value" "${DEVICE}"
  			(at 15.24 -82.55 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "8-Channel, 1000 Base-T Ethernet Transformer/Choke"
  			(at 0 0 0)
  		)
  		(symbol "XFMR_PULSE_HX5020FNL_1_0"
  			(text "CHANNEL 1"
  				(at 16.51 -1.27 0)
  			)
  			(text "CHANNEL 2"
  				(at 16.51 -11.43 0)
  			)
  			(text "CHANNEL 3"
  				(at 16.51 -21.59 0)
  			)
  			(text "CHANNEL 4"
  				(at 16.51 -31.75 0)
  			)
  			(text "CHANNEL 5"
  				(at 16.51 -41.91 0)
  			)
  			(text "CHANNEL 6"
  				(at 16.51 -52.07 0)
  			)
  			(text "CHANNEL 7"
  				(at 16.51 -62.23 0)
  			)
  			(text "CHANNEL 8"
  				(at 16.51 -72.39 0)
  			)
  			(pin bidirectional line
  				(at -5.08 -2.54 0)
  				(length 5.08)
  				(name "TD+")
  				(number "1")
  			)
  			(pin bidirectional line
  				(at -5.08 -5.08 0)
  				(length 5.08)
  				(name "TCT")
  				(number "2")
  			)
  			(pin bidirectional line
  				(at -5.08 -7.62 0)
  				(length 5.08)
  				(name "TD-")
  				(number "3")
  			)
  			(pin bidirectional line
  				(at -5.08 -12.7 0)
  				(length 5.08)
  				(name "TD+")
  				(number "4")
  			)
  			(pin bidirectional line
  				(at -5.08 -15.24 0)
  				(length 5.08)
  				(name "TCT")
  				(number "5")
  			)
  			(pin bidirectional line
  				(at -5.08 -17.78 0)
  				(length 5.08)
  				(name "TD-")
  				(number "6")
  			)
  			(pin bidirectional line
  				(at -5.08 -22.86 0)
  				(length 5.08)
  				(name "TD+")
  				(number "7")
  			)
  			(pin bidirectional line
  				(at -5.08 -25.4 0)
  				(length 5.08)
  				(name "TCT")
  				(number "8")
  			)
  			(pin bidirectional line
  				(at -5.08 -27.94 0)
  				(length 5.08)
  				(name "TD-")
  				(number "9")
  			)
  			(pin bidirectional line
  				(at -5.08 -33.02 0)
  				(length 5.08)
  				(name "TD+")
  				(number "10")
  			)
  			(pin bidirectional line
  				(at -5.08 -35.56 0)
  				(length 5.08)
  				(name "TCT")
  				(number "11")
  			)
  			(pin bidirectional line
  				(at -5.08 -38.1 0)
  				(length 5.08)
  				(name "TD-")
  				(number "12")
  			)
  			(pin bidirectional line
  				(at -5.08 -43.18 0)
  				(length 5.08)
  				(name "TD+")
  				(number "14")
  			)
  			(pin bidirectional line
  				(at -5.08 -45.72 0)
  				(length 5.08)
  				(name "TCT")
  				(number "15")
  			)
  			(pin bidirectional line
  				(at -5.08 -48.26 0)
  				(length 5.08)
  				(name "TD-")
  				(number "16")
  			)
  			(pin bidirectional line
  				(at -5.08 -53.34 0)
  				(length 5.08)
  				(name "TD+")
  				(number "17")
  			)
  			(pin bidirectional line
  				(at -5.08 -55.88 0)
  				(length 5.08)
  				(name "TCT")
  				(number "18")
  			)
  			(pin bidirectional line
  				(at -5.08 -58.42 0)
  				(length 5.08)
  				(name "TD-")
  				(number "19")
  			)
  			(pin bidirectional line
  				(at -5.08 -63.5 0)
  				(length 5.08)
  				(name "TD+")
  				(number "20")
  			)
  			(pin bidirectional line
  				(at -5.08 -66.04 0)
  				(length 5.08)
  				(name "TCT")
  				(number "21")
  			)
  			(pin bidirectional line
  				(at -5.08 -68.58 0)
  				(length 5.08)
  				(name "TD-")
  				(number "22")
  			)
  			(pin bidirectional line
  				(at -5.08 -73.66 0)
  				(length 5.08)
  				(name "TD+")
  				(number "23")
  			)
  			(pin bidirectional line
  				(at -5.08 -76.2 0)
  				(length 5.08)
  				(name "TCT")
  				(number "24")
  			)
  			(pin bidirectional line
  				(at -5.08 -78.74 0)
  				(length 5.08)
  				(name "TD-")
  				(number "25")
  			)
  			(pin bidirectional line
  				(at 35.56 -2.54 180)
  				(length 5.08)
  				(name "MX+")
  				(number "48")
  			)
  			(pin bidirectional line
  				(at 35.56 -5.08 180)
  				(length 5.08)
  				(name "MCT")
  				(number "49")
  			)
  			(pin bidirectional line
  				(at 35.56 -7.62 180)
  				(length 5.08)
  				(name "MX-")
  				(number "50")
  			)
  			(pin bidirectional line
  				(at 35.56 -12.7 180)
  				(length 5.08)
  				(name "MX+")
  				(number "47")
  			)
  			(pin bidirectional line
  				(at 35.56 -15.24 180)
  				(length 5.08)
  				(name "MCT")
  				(number "46")
  			)
  			(pin bidirectional line
  				(at 35.56 -17.78 180)
  				(length 5.08)
  				(name "MX-")
  				(number "45")
  			)
  			(pin bidirectional line
  				(at 35.56 -22.86 180)
  				(length 5.08)
  				(name "MX+")
  				(number "42")
  			)
  			(pin bidirectional line
  				(at 35.56 -25.4 180)
  				(length 5.08)
  				(name "MCT")
  				(number "43")
  			)
  			(pin bidirectional line
  				(at 35.56 -27.94 180)
  				(length 5.08)
  				(name "MX-")
  				(number "44")
  			)
  			(pin bidirectional line
  				(at 35.56 -33.02 180)
  				(length 5.08)
  				(name "MX+")
  				(number "41")
  			)
  			(pin bidirectional line
  				(at 35.56 -35.56 180)
  				(length 5.08)
  				(name "MCT")
  				(number "40")
  			)
  			(pin bidirectional line
  				(at 35.56 -38.1 180)
  				(length 5.08)
  				(name "MX-")
  				(number "39")
  			)
  			(pin bidirectional line
  				(at 35.56 -43.18 180)
  				(length 5.08)
  				(name "MX+")
  				(number "35")
  			)
  			(pin bidirectional line
  				(at 35.56 -45.72 180)
  				(length 5.08)
  				(name "MCT")
  				(number "36")
  			)
  			(pin bidirectional line
  				(at 35.56 -48.26 180)
  				(length 5.08)
  				(name "MX-")
  				(number "37")
  			)
  			(pin bidirectional line
  				(at 35.56 -53.34 180)
  				(length 5.08)
  				(name "MX+")
  				(number "34")
  			)
  			(pin bidirectional line
  				(at 35.56 -55.88 180)
  				(length 5.08)
  				(name "MCT")
  				(number "33")
  			)
  			(pin bidirectional line
  				(at 35.56 -58.42 180)
  				(length 5.08)
  				(name "MX-")
  				(number "32")
  			)
  			(pin bidirectional line
  				(at 35.56 -63.5 180)
  				(length 5.08)
  				(name "MX+")
  				(number "29")
  			)
  			(pin bidirectional line
  				(at 35.56 -66.04 180)
  				(length 5.08)
  				(name "MCT")
  				(number "30")
  			)
  			(pin bidirectional line
  				(at 35.56 -68.58 180)
  				(length 5.08)
  				(name "MX-")
  				(number "31")
  			)
  			(pin bidirectional line
  				(at 35.56 -73.66 180)
  				(length 5.08)
  				(name "MX+")
  				(number "28")
  			)
  			(pin bidirectional line
  				(at 35.56 -76.2 180)
  				(length 5.08)
  				(name "MCT")
  				(number "27")
  			)
  			(pin bidirectional line
  				(at 35.56 -78.74 180)
  				(length 5.08)
  				(name "MX-")
  				(number "26")
  			)
  		)
  		(embedded_fonts no)
  	)
)
