(footprint "XFMR_SCHAFFNER_IT243"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Pulse Transformer, Serie IT, Body 25.5mm x 25.5mm")
	(property "Reference" "REF**"
		(at 0 -9.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_SCHAFFNER_IT243"
		(at 0 9.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "1"
		(at -9.7 -5.953 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -9.7 -5.953 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -7.65 -6.25)
		(size 1.55 1.55)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 7.65 -6.25)
		(size 1.55 1.55)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at -7.65 -1.25)
		(size 1.55 1.55)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at 7.65 -1.25)
		(size 1.55 1.55)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -7.65 6.25)
		(size 1.55 1.55)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at 7.65 6.25)
		(size 1.55 1.55)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
