(footprint "XFMR_SCHAFFNER_IT248"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Pulse Transformer, Serie IT, Body 17.6mm x 16.7mm")
	(property "Reference" "REF**"
		(at 0 -9.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_SCHAFFNER_IT248"
		(at 0 9.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "1"
		(at -7.8 4.747 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "Prim."
		(at -2 -2.153 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -7.8 4.747 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Prim."
		(at -2 -2.153 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -7.65001 6.25 180)
		(size 1.4 1.4)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 7.65001 6.25 180)
		(size 1.4 1.4)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at -7.65001 -6.25 180)
		(size 1.4 1.4)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at 7.65001 -6.25 180)
		(size 1.4 1.4)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
