(footprint "XFMR_TALEMA_7000xK"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "1.6VA Toroidal Transformer, Body 39.6mm x 39.6mm, 70000 Serie")
	(property "Reference" "REF**"
		(at 0 -20.60525 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_TALEMA_7000xK"
		(at 0 20.60525 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "3"
		(at -14.075 -10.9025 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "5"
		(at -15.775 9.5975 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at -16.2 -8.2275 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "11"
		(at 10.675 14.4225 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "14"
		(at 10 -13.2525 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at -14.025 12.1725 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "13"
		(at 13.7 -9.5275 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "12"
		(at 13.425 11.2975 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "3" thru_hole circle
		(at -17.78001 -15.24001 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -17.78001 -10.16001 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -17.78001 10.16001 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at -17.78001 15.24001 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "11" thru_hole circle
		(at 17.78001 17.78001 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "12" thru_hole circle
		(at 17.78001 12.70001 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "13" thru_hole circle
		(at 17.78001 -12.70001 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "14" thru_hole circle
		(at 17.78001 -17.78001 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "MEC" thru_hole circle
		(at 0 0 180)
		(size 8 8)
		(drill 4.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
