(footprint "XFMR_TALEMA_7001xK"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "5VA Toroidal Transformer, Body 44.7mm x 44.7mm, 70000 Serie")
	(property "Reference" "REF**"
		(at 0 -23.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_TALEMA_7001xK"
		(at 0 23.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "4"
		(at -17.59999 -8.60299 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at -14.84999 14.12199 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "13"
		(at 13.54999 -11.52799 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "12"
		(at 14.09999 12.64699 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at -15.34999 -11.90299 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "14"
		(at 10.12499 -15.22799 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "11"
		(at 11.42499 15.97199 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "5"
		(at -17.14999 11.02199 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "3" thru_hole circle
		(at -20.36 -17.82 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -20.36 -12.74 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -20.36 12.74 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at -20.36 17.82 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "11" thru_hole circle
		(at 20.36 20.36 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "12" thru_hole circle
		(at 20.36 15.28 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "13" thru_hole circle
		(at 20.36 -15.28 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "14" thru_hole circle
		(at 20.36 -20.36 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "MEC" thru_hole circle
		(at 0 0 180)
		(size 8 8)
		(drill 4.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
