(footprint "XFMR_TALEMA_7003xK"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "7VA Toroidal Transformer, Body 49.7mm x 49.7mm, 70000 Serie")
	(property "Reference" "REF**"
		(at 0 -25.65001 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_TALEMA_7003xK"
		(at 0 25.65001 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "3"
		(at -17.85 -14.403 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at -17.35 16.622 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at -20.1 -11.103 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "5"
		(at -19.65 13.522 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "12"
		(at 16.6 15.147 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "13"
		(at 16.05 -14.028 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "14"
		(at 12.625 -17.728 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "11"
		(at 13.925 18.472 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "3" thru_hole circle
		(at -22.86001 -20.32001 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -22.86001 -15.24001 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -22.86001 15.24001 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at -22.86001 20.32001 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "11" thru_hole circle
		(at 22.86001 22.86001 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "12" thru_hole circle
		(at 22.86001 17.78001 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "13" thru_hole circle
		(at 22.86001 -17.78001 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "14" thru_hole circle
		(at 22.86001 -22.86001 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "MEC" thru_hole circle
		(at 0 0 180)
		(size 8 8)
		(drill 4.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
