(footprint "XFMR_TRIAD_CSE186L"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Audio Transformer- Body 10.41X7.87mm")
	(property "Reference" "REF**"
		(at 1 -11.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_TRIAD_CSE186L"
		(at 1 11.55 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "5" thru_hole circle
		(at 6.5 7.5 90)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at 6.5 2.5 90)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at 6.5 -2.5 90)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at 6.5 -7.5 90)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "A1" thru_hole circle
		(at -3.5 -6.3 90)
		(size 2.7 2.7)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "A2" thru_hole circle
		(at -1.5 5.2 90)
		(size 2.7 2.7)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
