(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "XFMR_WURTH_749020011A"
  		(pin_names
  			(offset 1.27)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "TR"
  			(at 16.51 1.27 0)
  		)
  		(property "Value" "${DEVICE}"
  			(at 16.51 -41.91 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "1000 Base-T LAN Transformer"
  			(at 0 0 0)
  		)
  		(symbol "XFMR_WURTH_749020011A_1_0"
  			(pin bidirectional line
  				(at -5.08 -2.54 0)
  				(length 5.08)
  				(name "TD1+")
  				(number "2")
  			)
  			(pin bidirectional line
  				(at -5.08 -5.08 0)
  				(length 5.08)
  				(name "TCT1")
  				(number "1")
  			)
  			(pin bidirectional line
  				(at -5.08 -7.62 0)
  				(length 5.08)
  				(name "TD1-")
  				(number "3")
  			)
  			(pin bidirectional line
  				(at -5.08 -12.7 0)
  				(length 5.08)
  				(name "TD2+")
  				(number "5")
  			)
  			(pin bidirectional line
  				(at -5.08 -15.24 0)
  				(length 5.08)
  				(name "TCT2")
  				(number "4")
  			)
  			(pin bidirectional line
  				(at -5.08 -17.78 0)
  				(length 5.08)
  				(name "TD2-")
  				(number "6")
  			)
  			(pin bidirectional line
  				(at -5.08 -22.86 0)
  				(length 5.08)
  				(name "TD3+")
  				(number "8")
  			)
  			(pin bidirectional line
  				(at -5.08 -25.4 0)
  				(length 5.08)
  				(name "TCT3")
  				(number "7")
  			)
  			(pin bidirectional line
  				(at -5.08 -27.94 0)
  				(length 5.08)
  				(name "TD3-")
  				(number "9")
  			)
  			(pin bidirectional line
  				(at -5.08 -33.02 0)
  				(length 5.08)
  				(name "TD4+")
  				(number "11")
  			)
  			(pin bidirectional line
  				(at -5.08 -35.56 0)
  				(length 5.08)
  				(name "TCT4")
  				(number "10")
  			)
  			(pin bidirectional line
  				(at -5.08 -38.1 0)
  				(length 5.08)
  				(name "TD4-")
  				(number "12")
  			)
  			(pin bidirectional line
  				(at 38.1 -2.54 180)
  				(length 5.08)
  				(name "MX1+")
  				(number "23")
  			)
  			(pin bidirectional line
  				(at 38.1 -5.08 180)
  				(length 5.08)
  				(name "MCT1")
  				(number "24")
  			)
  			(pin bidirectional line
  				(at 38.1 -7.62 180)
  				(length 5.08)
  				(name "MX1-")
  				(number "22")
  			)
  			(pin bidirectional line
  				(at 38.1 -12.7 180)
  				(length 5.08)
  				(name "MX2+")
  				(number "20")
  			)
  			(pin bidirectional line
  				(at 38.1 -15.24 180)
  				(length 5.08)
  				(name "MCT2")
  				(number "21")
  			)
  			(pin bidirectional line
  				(at 38.1 -17.78 180)
  				(length 5.08)
  				(name "MX2-")
  				(number "19")
  			)
  			(pin bidirectional line
  				(at 38.1 -22.86 180)
  				(length 5.08)
  				(name "MX3+")
  				(number "17")
  			)
  			(pin bidirectional line
  				(at 38.1 -25.4 180)
  				(length 5.08)
  				(name "MCT3")
  				(number "18")
  			)
  			(pin bidirectional line
  				(at 38.1 -27.94 180)
  				(length 5.08)
  				(name "MX3-")
  				(number "16")
  			)
  			(pin bidirectional line
  				(at 38.1 -33.02 180)
  				(length 5.08)
  				(name "MX4+")
  				(number "14")
  			)
  			(pin bidirectional line
  				(at 38.1 -35.56 180)
  				(length 5.08)
  				(name "MCT4")
  				(number "15")
  			)
  			(pin bidirectional line
  				(at 38.1 -38.1 180)
  				(length 5.08)
  				(name "MX4-")
  				(number "13")
  			)
  		)
  		(embedded_fonts no)
  	)
)
