(footprint "XFMR_WURTH_EFD25"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "WE-FB Flyback Transformer, Body 32.31 x 27.03mm, Size EFD25")
	(property "Reference" "REF**"
		(at 0.00004 -14.47501 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_WURTH_EFD25"
		(at 0.00004 14.47501 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -15.18997 -9.4)
		(size 2.5 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -15.18997 -5.64)
		(size 2.5 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -15.18997 -1.88)
		(size 2.5 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -15.18997 1.88)
		(size 2.5 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -15.18997 5.64)
		(size 2.5 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -15.18997 9.4)
		(size 2.5 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 15.19005 9.4)
		(size 2.5 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 15.19005 5.64)
		(size 2.5 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 15.19005 1.88)
		(size 2.5 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 15.19005 -1.88)
		(size 2.5 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 15.19005 -5.64)
		(size 2.5 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 15.19005 -9.4)
		(size 2.5 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
