(footprint "XFMR_WURTH_MID-OLEFD EFD20 SMT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "MID-OLEFD Flyback Transformer, Body 33.8 x 21.5mm, Style EFD20 SMT")
	(property "Reference" "REF**"
		(at 0 -11.725 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_WURTH_MID-OLEFD EFD20 SMT"
		(at 0 11.725 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -15.36 -7.5)
		(size 3.05 1.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -15.36 -4.5)
		(size 3.05 1.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -15.36 -1.5)
		(size 3.05 1.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -15.36 1.5)
		(size 3.05 1.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -15.36 4.5)
		(size 3.05 1.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -15.36 7.5)
		(size 3.05 1.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 15.36 7.5)
		(size 3.05 1.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 15.36 4.5)
		(size 3.05 1.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 15.36 1.5)
		(size 3.05 1.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 15.36 -1.5)
		(size 3.05 1.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 15.36 -4.5)
		(size 3.05 1.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 15.36 -7.5)
		(size 3.05 1.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
