(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Conn_BNC_031-70526-21"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 20.32 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Conn_BNC_031-70526-21"
				(at 20.32 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Conn_BNC_031-70526-21"
				(at 20.32 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.farnell.com/cad/2305565.pdf?_ga=2.190633003.1014497200.1574067480-156563690.1566371002&_gac=1.57062104.1572875319.Cj0KCQiAtf_tBRDtARIsAIbAKe0A1M5y_jdFCiNLNrHM5L2GjmDvn_4qnRvhHAD9jBdL9AmoMNThLCoaAjhJEALw_wcB"
				(at 20.32 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF / Coaxial Connector, BNC Coaxial, Straight Bulkhead Jack, Board Edge / End Launch, 75 ohm"
				(at 20.32 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "031-70526-21"
				(at 20.32 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Amphenol"
				(at 20.32 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 20.32 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 20.32 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "HORIZONTAL, BULKHEAD, RF, CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "*BNC* *SMA* *SMB* *SMC* *Cinch*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Conn_BNC_031-70526-21_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 5.08 -5.08 90)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
)
