(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "RJ45_1149611"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "RJ45_1149611"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "RJ45_1149611"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.tme.eu/Document/8ba1d1eb57ed3008041998d6d3ae847f/1149611.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Jack Modular Connector 8p8c (RJ45, Ethernet) Vertical Unshielded"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Phoenix Contact"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "1149611"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "RJ45_1149611_1_1"
				(pin passive line
					(at 0 0 270)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 2.54 0 270)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 5.08 0 270)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin passive line
					(at 7.62 0 270)
					(length 2.54)
					(name "")
					(number "4")
				)
				(pin passive line
					(at 10.16 0 270)
					(length 2.54)
					(name "")
					(number "5")
				)
				(pin passive line
					(at 12.7 0 270)
					(length 2.54)
					(name "")
					(number "6")
				)
				(pin passive line
					(at 15.24 0 270)
					(length 2.54)
					(name "")
					(number "7")
				)
				(pin passive line
					(at 17.78 0 270)
					(length 2.54)
					(name "")
					(number "8")
				)
				(pin passive line
					(at 22.86 -19.05 180)
					(length 2.54)
					(name "")
					(number "SH")
				)
			)
			(embedded_fonts no)
		)
)
