(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "FFC_TE_1734742-6"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 21.59 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "FFC_TE_1734742-6"
				(at 21.59 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "FFC_TE_1734742-6"
				(at 21.59 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/418/7/ENG_CD_1734742_P-2017175.pdf"
				(at 21.59 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "FFC & FPC Connectors .5 FPC VT ZIF Type-A 6 contacts"
				(at 21.59 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "1734742-6"
				(at 21.59 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "TE Connectivity"
				(at 21.59 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 21.59 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 21.59 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "FFC_TE_1734742-6_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "")
					(number "4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "")
					(number "5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "")
					(number "6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "MP")
					(number "MP")
				)
			)
			(embedded_fonts no)
		)
)
