(footprint "USB-Micro-B_Receptacle_Molex_473460001"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "http://www.molex.com/pdm_docs/sd/473460001_sd.pdf")
	(property "Reference" "REF**"
		(at 0 -3.376 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB-Micro-B_Receptacle_Molex_473460001"
		(at 0 3.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -7.925 5.975 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -7.925 7.175 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -7.925 9.575 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.301 -2.376 90)
		(size 1.38 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.652 -2.376 90)
		(size 1.38 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -0.001 -2.376 90)
		(size 1.38 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.652 -2.376 90)
		(size 1.38 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.3 -2.376 90)
		(size 1.38 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -2.911 0.284 90)
		(size 1.9 2.375)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -2.464 -2.016 90)
		(size 2.1 1.475)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -0.836 0.284 90)
		(size 1.9 1.175)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 0.836 0.284 90)
		(size 1.9 1.175)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 2.463 -2.016 90)
		(size 2.1 1.475)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 2.913 0.284 90)
		(size 1.9 2.375)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_473460001.glb"
		(offset
			(xyz -0.001 0.036 1.2)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
