(footprint "Conn_FFC_Molex_5019510550"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Footprint based on: https://www.molex.com/content/dam/molex/molex-dot-com/products/automated/en-us/salesdrawingpdf/501/501951/5019510550_sd.pdf?inline")
	(tags "Connector")
	(property "Reference" "REF**"
		(at 0 -2.97 0)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_FFC_Molex_5019510550"
		(at 0 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at -0.123 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at -0.123 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -2.9 4.9 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -2.9 6.1 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -2.9 7.3 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.575 -1 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.325 -0.5 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.575 0 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 1.325 0.5 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.575 1 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at -1.475 -2 270)
		(size 0.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at -1.475 2 270)
		(size 0.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at 1.225 -2 270)
		(size 0.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at 1.225 2 270)
		(size 0.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_501951_0550.glb"
		(offset
			(xyz -0.14 0 0.52)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 90)
		)
	)
)
