(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "D-Sub_TE_5747840-3"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 26.67 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "D-Sub_TE_5747840-3"
				(at 26.67 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "D-Sub_TE_5747840-3"
				(at 26.67 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=5747840&DocType=Customer+Drawing&DocLang=English"
				(at 26.67 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "9 Position D-Sub Plug, Male Pins Connector"
				(at 26.67 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "5747840-3"
				(at 26.67 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "TE Connectivity"
				(at 26.67 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 26.67 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 26.67 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, VIDEO, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "D-Sub_TE_5747840-3_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "")
					(number "4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "")
					(number "5")
				)
				(pin passive line
					(at 12.7 -1.27 180)
					(length 2.54)
					(name "")
					(number "6")
				)
				(pin passive line
					(at 12.7 -3.81 180)
					(length 2.54)
					(name "")
					(number "7")
				)
				(pin passive line
					(at 12.7 -6.35 180)
					(length 2.54)
					(name "")
					(number "8")
				)
				(pin passive line
					(at 12.7 -8.89 180)
					(length 2.54)
					(name "")
					(number "9")
				)
				(pin passive line
					(at 12.7 -11.43 180)
					(length 2.54)
					(name "SH")
					(number "10")
				)
			)
			(embedded_fonts no)
		)
)
