(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "WE_MicroSIM_Hinge_693022010811"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "WE_MicroSIM_Hinge_693022010811"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "WE_MicroSIM_Hinge_693022010811"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.we-online.com/components/products/datasheet/693022010811.pdf"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "8 Position Card Connector Micro SIM Surface Mount, Right Angle Gold"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "693022010811"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Würth Elektronik"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "WE_MicroSIM_Hinge_693022010811_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "C1")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 2.54)
					(name "RST")
					(number "C2")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 2.54)
					(name "CLK")
					(number "C3")
				)
				(pin no_connect line
					(at 22.86 -7.62 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "C4")
				)
				(pin power_in line
					(at 25.4 -16.51 180)
					(length 2.54)
					(name "GND")
					(number "C5")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VPP")
					(number "C6")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 2.54)
					(name "I/O")
					(number "C7")
				)
				(pin no_connect line
					(at 22.86 -10.16 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "C8")
				)
				(pin passive line
					(at 25.4 -16.51 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "Z1")
				)
				(pin passive line
					(at 25.4 -16.51 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "Z2")
				)
			)
			(embedded_fonts no)
		)
)
