(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "L834-1G1T-S7"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "L834-1G1T-S7"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "L834-1G1T-S7"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.belfuse.com/resources/drawings/magneticsolutions/dr-mag-l834-1g1t-s7.pdf"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Modular connector with magnetics"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "L834-1G1T-S7"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Bel Fuse"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "HORIZONTAL, THT, FILTERED, CONNECTOR, ETHERNET"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "L834-1G1T-S7_0_0"
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "TRCT3")
					(number "1")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "TRD3-")
					(number "2")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "TRD3+")
					(number "3")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 2.54)
					(name "TRD2+")
					(number "4")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 2.54)
					(name "TRD2-")
					(number "5")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "TRCT2")
					(number "6")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "TRCT4")
					(number "7")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 2.54)
					(name "TRD4+")
					(number "8")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 2.54)
					(name "TRD4-")
					(number "9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "TRD1-")
					(number "10")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "TRD1+")
					(number "11")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "TRCT1")
					(number "12")
				)
				(pin passive line
					(at 17.78 -7.62 180)
					(length 2.54)
					(name "")
					(number "13")
				)
				(pin passive line
					(at 17.78 -3.81 180)
					(length 2.54)
					(name "")
					(number "14")
				)
				(pin passive line
					(at 17.78 -30.48 180)
					(length 2.54)
					(name "SH")
					(number "SH")
				)
			)
			(symbol "L834-1G1T-S7_1_1"
				(text "G"
					(at 13.208 -15.621 0)
				)
				(text "G"
					(at 13.335 -6.731 0)
				)
				(pin passive line
					(at 17.78 -16.51 180)
					(length 2.54)
					(name "")
					(number "15")
				)
				(pin passive line
					(at 17.78 -12.7 180)
					(length 2.54)
					(name "")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
