(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "BarrelJack_Pin2.5mm_PJ-063BH"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 17.78 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "BarrelJack_Pin2.5mm_PJ-063BH"
				(at 17.78 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "BarrelJack_Pin2.5mm_PJ-063BH"
				(at 17.78 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/670/pj_063bh-1778662.pdf"
				(at 17.78 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Power Barrel Connector Jack 2.5mm ID (0.098\"), 5.50mm OD (0.217\") Through Hole, Right Angle"
				(at 17.78 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PJ-063BH"
				(at 17.78 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "CUI Inc"
				(at 17.78 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 17.78 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 17.78 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, POWER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "BarrelJack_Pin2.5mm_PJ-063BH_1_1"
				(pin passive line
					(at 2.54 0 180)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 2.54 -2.54 180)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 2.54 -5.08 180)
					(length 2.54)
					(name "")
					(number "SH")
				)
			)
			(embedded_fonts no)
		)
)
