(footprint "Tag-Connect_TC2030-IDC-NL_2x3_P1.27mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Tag-Connect programming header")
	(tags "tag connect programming header pogo pins")
	(property "Reference" "REF**"
		(at 0 -3.05 0)
		(layer "F.SilkS")
	)
	(property "Value" "Tag-Connect_TC2030-IDC-NL_2x3_P1.27mm"
		(at -2.5 2.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_bom)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "KEEPOUT"
		(at 1.267 -0.634 0)
		(layer "Cmts.User")
	)
	(fp_text user "License: Apache-2.0"
		(at -2.6 6.55 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -2.584 4.063 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -2.584 5.264 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -1.27 -0.64)
		(size 0.9906 0.9906)
		(drill 0.9906)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.809 -1.651)
		(size 0.9906 0.9906)
		(drill 0.9906)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.809 0.377)
		(size 0.9906 0.9906)
		(drill 0.9906)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" connect circle
		(at 0 0)
		(size 0.7874 0.7874)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" connect circle
		(at 0 -1.27)
		(size 0.7874 0.7874)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" connect circle
		(at 1.267 0)
		(size 0.7874 0.7874)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" connect circle
		(at 1.267 -1.27)
		(size 0.7874 0.7874)
		(layers "F.Cu" "F.Mask")
	)
	(pad "5" connect circle
		(at 2.536 0)
		(size 0.7874 0.7874)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" connect circle
		(at 2.536 -1.27)
		(size 0.7874 0.7874)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "antmicro_tc2030_idc_nl.glb"
		(offset
			(xyz 1.6 -0.53 24)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 90)
		)
	)
)
