(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Tag-Connect_TC2030-IDC-NL_2x3_P1.27mm"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 26.67 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Tag-Connect_TC2030-IDC-NL_2x3_P1.27mm"
				(at 26.67 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Tag-Connect_TC2030-IDC-NL_2x3_P1.27mm"
				(at 26.67 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Tag-Connect/TC2030-IDC_RevB.pdf"
				(at 26.67 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Tag Connect 2x3 1.27mm terminal"
				(at 26.67 -22.225 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TC2030-IDC-NL"
				(at 26.67 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Tag Connect"
				(at 26.67 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 26.67 -17.145 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 26.67 -19.685 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "POGO-PIN, CONNECTOR"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Tag-Connect_TC2030-IDC-NL_2x3_P1.27mm_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 12.7 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "3")
					(number "3")
				)
				(pin passive line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "4")
					(number "4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "5")
					(number "5")
				)
				(pin passive line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "6")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
