(footprint "Tag-Connect_TC2050-IDC-NL_2x5_P1.27mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Tag-Connect_TC2050-IDC-NL_2x5_P1.27mm"
		(at 0 4.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Z-KEEPOUT 6.35mm"
		(at -2.2 2.8 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at -6.223 6.049 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -6.223 7.249 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -6.223 8.449 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -3.81 0)
		(size 0.9906 0.9906)
		(drill 0.9906)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.809 -1.016)
		(size 0.9906 0.9906)
		(drill 0.9906)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.809 1.015)
		(size 0.9906 0.9906)
		(drill 0.9906)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" connect circle
		(at -2.54 0.634)
		(size 0.7874 0.7874)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" connect circle
		(at -1.27 0.634)
		(size 0.7874 0.7874)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" connect circle
		(at 0 0.634)
		(size 0.7874 0.7874)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" connect circle
		(at 1.269 0.634)
		(size 0.7874 0.7874)
		(layers "F.Cu" "F.Mask")
	)
	(pad "5" connect circle
		(at 2.539 0.634)
		(size 0.7874 0.7874)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" connect circle
		(at 2.539 -0.635)
		(size 0.7874 0.7874)
		(layers "F.Cu" "F.Mask")
	)
	(pad "7" connect circle
		(at 1.269 -0.635)
		(size 0.7874 0.7874)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" connect circle
		(at 0 -0.635)
		(size 0.7874 0.7874)
		(layers "F.Cu" "F.Mask")
	)
	(pad "9" connect circle
		(at -1.27 -0.635)
		(size 0.7874 0.7874)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" connect circle
		(at -2.54 -0.635)
		(size 0.7874 0.7874)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
)
