(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "1N5806U01A"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "D"
				(at 22.86 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "1N5806U01A"
				(at 22.86 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "1N5806U01A"
				(at 22.86 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.st.com/resource/en/datasheet/1n5806u.pdf"
				(at 22.86 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Aerospace 150 V, 2.5 A ultrafast rectifier in LCC-2A package"
				(at 22.86 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "1N5806U01A"
				(at 22.86 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "STMicroelectronics"
				(at 22.86 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 22.86 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 22.86 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, RECTIFIER, SEMICONDUCTOR, DIODE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "1N5806U01A_0_1")
			(symbol "1N5806U01A_1_1"
				(pin passive line
					(at 5.08 0 180)
					(length 0.635)
					(name "A")
					(number "1")
				)
				(pin passive line
					(at 0 0 0)
					(length 0.635)
					(name "C")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
)
