(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "824013"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "D"
				(at 30.48 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "824013"
				(at 30.48 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "824013"
				(at 30.48 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://docs.rs-online.com/cc4f/0900766b8107e9d4.pdf"
				(at 30.48 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "TVS diode array, SOT-23-6, 3.3 V, 3 pF"
				(at 30.48 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "824013"
				(at 30.48 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Würth Elektronik"
				(at 30.48 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 30.48 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "DIODE, SEMICONDUCTOR, TVS, ESD, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "SOT?23*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "824013_0_1")
			(symbol "824013_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin power_in line
					(at 0 -3.81 0)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin passive line
					(at 16.51 -7.62 180)
					(length 2.54)
					(name "")
					(number "4")
				)
				(pin power_in line
					(at 16.51 -3.81 180)
					(length 2.54)
					(name "")
					(number "5")
				)
				(pin passive line
					(at 16.51 0 180)
					(length 2.54)
					(name "")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
