(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ACPL-247-560E"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 25.4 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ACPL-247-560E"
				(at 25.4 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ACPL-247-560E"
				(at 25.4 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/678/avgo_s_a0004682437_1-2291080.pdf"
				(at 25.4 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DC Input, Multi-Channel Half-Pitch Phototransistor Optocoupler"
				(at 25.4 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Broadcom"
				(at 25.4 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ACPL-247-560E"
				(at 25.4 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 25.4 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 25.4 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, OPTOCOUPLER, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ACPL-247-560E_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "")
					(number "4")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "")
					(number "5")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "")
					(number "6")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "")
					(number "7")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "")
					(number "8")
				)
				(pin passive line
					(at 12.7 -27.94 180)
					(length 2.54)
					(name "")
					(number "9")
				)
				(pin passive line
					(at 12.7 -22.86 180)
					(length 2.54)
					(name "")
					(number "10")
				)
				(pin passive line
					(at 12.7 -20.32 180)
					(length 2.54)
					(name "")
					(number "11")
				)
				(pin passive line
					(at 12.7 -15.24 180)
					(length 2.54)
					(name "")
					(number "12")
				)
				(pin passive line
					(at 12.7 -12.7 180)
					(length 2.54)
					(name "")
					(number "13")
				)
				(pin passive line
					(at 12.7 -7.62 180)
					(length 2.54)
					(name "")
					(number "14")
				)
				(pin passive line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "")
					(number "15")
				)
				(pin passive line
					(at 12.7 0 180)
					(length 2.54)
					(name "")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
