(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "B360A-M3"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "D"
				(at 21.59 -1.905 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "B360A-M3"
				(at 21.59 -12.065 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "B360A-M3"
				(at 21.59 -6.985 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.vishay.com/docs/89414/b350a-m3.pdf"
				(at 21.59 -9.525 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Schottky Rectifier, 60 V, 3 A, Single, SMA, 2 Pins, 720 mV"
				(at 21.59 -22.225 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 21.59 -17.145 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 21.59 -19.685 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, RECTIFIER, SEMICONDUCTOR, DIODE, SCHOTTKY, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "B360A-M3_0_1")
			(symbol "B360A-M3_1_1"
				(pin passive line
					(at 0 0 0)
					(length 0.635)
					(name "C")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 0.635)
					(name "A")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
)
