(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "BAT54A"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "D"
				(at 22.86 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "BAT54A"
				(at 22.86 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "BAT54A"
				(at 22.86 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://diotec.com/request/datasheet/bat54.pdf"
				(at 22.86 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Small Signal Schottky Diode, Dual Common Anode, 30 V, 200 mA, 500 mV, 600 mA, 150 °C"
				(at 22.86 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "BAT54A"
				(at 22.86 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Diotec Semiconductor"
				(at 22.86 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 22.86 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 22.86 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, SEMICONDUCTOR, DIODE, SCHOTTKY, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "BAT54A_0_1")
			(symbol "BAT54A_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "3")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
)
