(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "BAT54C-E3-08"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "D"
				(at 29.21 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "BAT54C-E3-08"
				(at 29.21 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "BAT54C-E3-08"
				(at 29.21 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.vishay.com/docs/86410/bat54_bat54a_bat54c_bat54s.pdf"
				(at 29.21 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Small Signal Schottky Diode, Dual Common Cathode, 30 V, 200 mA, 800 mV, 600 mA, 125 °C"
				(at 29.21 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Vishay"
				(at 29.21 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "BAT54C-E3-08"
				(at 29.21 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 29.21 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 29.21 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, SEMICONDUCTOR, DIODE, SCHOTTKY, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "BAT54C-E3-08_0_1")
			(symbol "BAT54C-E3-08_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "3")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
)
