(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "BCM857BS-7-F"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Q"
				(at 22.86 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "BCM857BS-7-F"
				(at 22.86 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "BCM857BS-7-F"
				(at 22.86 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.diodes.com/assets/Datasheets/BCM857BS.pdf"
				(at 22.86 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Bipolar (BJT) Transistor Array, 2 Transistors, PNP, 45V, 100mA, SOT-363, Surface Mount"
				(at 22.86 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "BCM857BS-7-F"
				(at 22.86 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Diodes Incorporated"
				(at 22.86 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 22.86 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 22.86 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, TRANSISTOR, SEMICONDUCTOR, BIPOLAR"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "BCM857BS-7-F_1_1"
				(pin passive line
					(at 6.35 -6.35 90)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 11.43 6.35 270)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin passive line
					(at 11.43 -6.35 90)
					(length 2.54)
					(name "")
					(number "4")
				)
				(pin input line
					(at 17.78 0 180)
					(length 2.54)
					(name "")
					(number "5")
				)
				(pin passive line
					(at 6.35 6.35 270)
					(length 2.54)
					(name "")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
