(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "BSC021N08NS5"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Q"
				(at 22.86 2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "BSC021N08NS5"
				(at 22.86 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "BSC021N08NS5"
				(at 22.86 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.infineon.com/assets/row/public/documents/24/49/infineon-bsc021n08ns5-datasheet-en.pdf?fileId=5546d462689a790c0168c7cb2946643e"
				(at 22.86 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "OptiMOS, N Channel, 80 V,  226A, 2.1 mOhm, Surface Mount"
				(at 22.86 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "BSC021N08NS5ATMA1"
				(at 22.86 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Infineon"
				(at 22.86 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 22.86 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 22.86 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MOSFET, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "BSC021N08NS5_1_1"
				(pin passive line
					(at 7.62 -3.81 90)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "4")
				)
				(pin passive line
					(at 7.62 8.89 270)
					(length 2.54)
					(name "")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
