(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "DMPH4029LFGQ"
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Q"
				(at 13.97 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "DMPH4029LFGQ"
				(at 13.97 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "DMPH4029LFGQ"
				(at 13.97 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMPH4029LFGQ.pdf"
				(at 13.97 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Power MOSFET, P Channel, 40 V, 22 A, 0.018 ohm, PowerDI 3333, Surface Mount"
				(at 13.97 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "DMPH4029LFGQ-7"
				(at 13.97 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Diodes Incorporated"
				(at 13.97 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 13.97 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 13.97 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, TRANSISTOR, SEMICONDUCTOR, MOSFET, PMOS, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "DMPH4029LFGQ_1_1"
				(pin passive line
					(at 7.62 -3.81 90)
					(length 2.54)
					(name "S")
					(number "1")
				)
				(pin passive line
					(at 7.62 -3.81 90)
					(length 2.54)
					(hide yes)
					(name "S")
					(number "2")
				)
				(pin passive line
					(at 7.62 -3.81 90)
					(length 2.54)
					(hide yes)
					(name "S")
					(number "3")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "G")
					(number "4")
				)
				(pin passive line
					(at 7.62 8.89 270)
					(length 2.54)
					(name "D")
					(number "5")
				)
			)
			(embedded_fonts no)
		)
)
