(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "EPC7020GSH"
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Q"
				(at 10.922 0.508 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "EPC7020GSH"
				(at 10.922 -9.652 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "EPC7020GSH"
				(at 10.922 -4.572 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://epc.space/documents/datasheets/EPC7020G-datasheet.pdf"
				(at 10.922 -7.112 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "200 V, 14.5 mΩ, 200 A pulsed radiation-hardened GaN"
				(at 10.922 -19.812 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "EPC7020GSH"
				(at 10.922 -2.032 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "EPC Space"
				(at 10.922 -12.192 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 10.922 -14.732 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 10.922 -17.272 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, TRANSISTOR, SEMICONDUCTOR, GAN, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "EPC7020GSH_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "G")
					(number "1")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "G")
					(number "2")
				)
				(pin passive line
					(at 7.62 6.35 270)
					(length 2.54)
					(name "D")
					(number "3")
				)
				(pin passive line
					(at 7.62 -6.35 90)
					(length 2.54)
					(name "S")
					(number "4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SS")
					(number "5")
				)
			)
			(embedded_fonts no)
		)
)
