(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ESD5B5_0ST1G"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "D"
				(at 25.4 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ESD5B5_0ST1G"
				(at 25.4 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ESD5B5_0ST1G"
				(at 25.4 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/esd5b5.0st1-d.pdf"
				(at 25.4 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Bidirectional TVS, 30 kV,  SOD-523, 5 V, 32 pF"
				(at 25.4 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 25.4 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 25.4 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "DIODE, SEMICONDUCTOR, TVS, ESD, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ESD5B5_0ST1G_0_0"
				(text ""
					(at 7.62 -1.27 0)
				)
			)
			(symbol "ESD5B5_0ST1G_0_1")
			(symbol "ESD5B5_0ST1G_1_1"
				(pin passive line
					(at 0 0 0)
					(length 0.635)
					(name "C")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 0.635)
					(name "A")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
)
