(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "FZT605TA"
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Q"
				(at 26.67 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "FZT605TA"
				(at 26.67 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "FZT605TA"
				(at 26.67 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.diodes.com/assets/Datasheets/FZT605.pdf"
				(at 26.67 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Darlington Transistor, NPN, 120V, 1.5A, 1.2W, SOT-223, Surface Mount"
				(at 26.67 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "FZT605TA"
				(at 26.67 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Diodes Incorporated"
				(at 26.67 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 26.67 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 26.67 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, TRANSISTOR, SEMICONDUCTOR, BIPOLAR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "SOT?323*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "FZT605TA_0_1")
			(symbol "FZT605TA_1_1"
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "B")
					(number "1")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "C")
					(number "2")
				)
				(pin passive line
					(at 17.78 -11.43 180)
					(length 2.54)
					(name "E")
					(number "3")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "C")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
)
