(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LED_Matrix_KWM-50571AGB"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 43.18 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LED_Matrix_KWM-50571AGB"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LED_Matrix_KWM-50571AGB"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.luckylight.cn/media/component/data-sheet/KWM-50571AGB.pdf"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "7.62mm 5×7 Super Yellow Green Dot Matrix LED Display"
				(at 43.18 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "KWM-50571AGB"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Luckylight"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "LED, THT, MODULE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LED_Matrix_KWM-50571AGB_1_1"
				(text "C1"
					(at 6.096 1.778 0)
				)
				(text "C2"
					(at 9.398 1.778 0)
				)
				(text "C3"
					(at 12.446 1.778 0)
				)
				(text "C4"
					(at 15.748 1.778 0)
				)
				(text "C5"
					(at 18.796 1.778 0)
				)
				(text "Cx"
					(at 24.13 -17.018 0)
				)
				(text "Ay"
					(at 24.384 -12.446 0)
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "A5")
					(number "1")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "A7")
					(number "2")
				)
				(pin passive line
					(at 29.21 -2.54 180)
					(length 2.54)
					(name "C2")
					(number "3")
				)
				(pin passive line
					(at 29.21 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "C3")
					(number "4")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "A4")
					(number "5")
				)
				(pin passive line
					(at 29.21 -10.16 180)
					(length 2.54)
					(name "C5")
					(number "6")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "A6")
					(number "7")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "A3")
					(number "8")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "A1")
					(number "9")
				)
				(pin passive line
					(at 29.21 -7.62 180)
					(length 2.54)
					(name "C4")
					(number "10")
				)
				(pin passive line
					(at 29.21 -5.08 180)
					(length 2.54)
					(name "C3")
					(number "11")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "A4")
					(number "12")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 2.54)
					(name "C1")
					(number "13")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "A2")
					(number "14")
				)
			)
			(embedded_fonts no)
		)
)
