(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PJA3441"
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Q"
				(at 20.32 6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PJA3441"
				(at 20.32 3.81 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PJA3441"
				(at 20.32 1.27 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/1057/PJA3441-1867252.pdf"
				(at 20.32 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "MOSFET, P Channel, 40V, 3.1A, 0.108 ohm, SOT-23, Surface Mount"
				(at 20.32 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PJA3441_R1_00001"
				(at 20.32 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "PANJIT"
				(at 20.32 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 20.32 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 20.32 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, TRANSISTOR, SEMICONDUCTOR, MOSFET, PMOS, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PJA3441_1_1"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "G")
					(number "1")
				)
				(pin passive line
					(at 6.35 -2.54 90)
					(length 2.54)
					(name "S")
					(number "2")
				)
				(pin passive line
					(at 6.35 7.62 270)
					(length 2.54)
					(name "D")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
)
