(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PJE138K"
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Q"
				(at 22.86 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PJE138K"
				(at 22.86 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PJE138K"
				(at 22.86 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/1057/PJE138K-1876698.pdf"
				(at 22.86 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "MOSFET, N Channel, 50V, 0.35A, 4.5 ohm, SOT-523, Surface Mount"
				(at 22.86 -26.67 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PJE138K_R1_00001"
				(at 22.86 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "PANJIT"
				(at 22.86 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 22.86 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 22.86 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, TRANSISTOR, SEMICONDUCTOR, MOSFET, NMOS, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PJE138K_1_1"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "G")
					(number "1")
				)
				(pin passive line
					(at 6.35 -2.54 90)
					(length 2.54)
					(name "S")
					(number "2")
				)
				(pin passive line
					(at 6.35 7.62 270)
					(length 2.54)
					(name "D")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
)
