(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "BC807-25W"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Q"
				(at 17.018 2.794 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "BC807-25W"
				(at 17.018 0.254 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "BC807-25W"
				(at 17.018 -2.286 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/308/BC807_25W_D-2310030.pdf"
				(at 17.018 -4.826 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Bipolar (BJT) Single Transistor, PNP, 45 V, 500 mA, 460 mW, SC-70, Surface Mount"
				(at 17.018 -17.526 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SBC807-40WT1G"
				(at 17.018 -7.366 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "ON Semiconductor"
				(at 17.018 -9.906 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 17.018 -12.446 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 17.018 -14.986 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, TRANSISTOR, SEMICONDUCTOR, PNP, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "BC807-25W_1_1"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 6.35 -5.08 90)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 6.35 5.08 270)
					(length 2.54)
					(name "")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
)
