(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SI4401BDY-T1-E3"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Q"
				(at 22.86 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SI4401BDY-T1-E3"
				(at 22.86 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SI4401BDY-T1-E3"
				(at 22.86 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.vishay.com/docs/73140/si4401bd.pdf"
				(at 22.86 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Power MOSFET, PChannel, 40 V, 8.7 A, 0.021ohm, SO-8, Surface Mount"
				(at 22.86 -26.67 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SI4401BDY-T1-E3"
				(at 22.86 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Vishay"
				(at 22.86 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 22.86 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 22.86 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, TRANSISTOR, SEMICONDUCTOR, MOSFET, PMOS, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SI4401BDY-T1-E3_1_1"
				(pin passive line
					(at 7.62 -3.81 90)
					(length 2.54)
					(name "S")
					(number "1")
				)
				(pin passive line
					(at 7.62 -3.81 90)
					(length 2.54)
					(hide yes)
					(name "S")
					(number "2")
				)
				(pin passive line
					(at 7.62 -3.81 90)
					(length 2.54)
					(hide yes)
					(name "S")
					(number "3")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "G")
					(number "4")
				)
				(pin passive line
					(at 7.62 8.89 270)
					(length 2.54)
					(name "D")
					(number "5")
				)
				(pin passive line
					(at 7.62 8.89 270)
					(length 2.54)
					(hide yes)
					(name "D")
					(number "6")
				)
				(pin passive line
					(at 7.62 8.89 270)
					(length 2.54)
					(hide yes)
					(name "D")
					(number "7")
				)
				(pin passive line
					(at 7.62 8.89 270)
					(length 2.54)
					(hide yes)
					(name "D")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
